Device Setting
Connection settings | IP address Port Device ID Encryption Enable buffer |

Console

ePOS SDK Display Object
Window(createWindow) | Define display area | Window No. X-coordinate Y-coordinate Width Height Scroll Mode |
Discard display area setting | Window No. to discard |
Switch display area | Window No. to move |
Clear current display area |  |
Cursor | Set cursor position | X-coodinate Y-coodinate |
Move cursor position in current window |  |
Cursor Type |  |
Text | Display text | String Language X-coordinate Y-coordinate R G B |
Display inverted text | String Language X-coordinate Y-coordinate |
Display marquee | String Format Display interval(100～2,000)(ms) Repeat interval(100～2,000)(ms) Repeat count(0～127) Language |
Properties | Blinking display | Blinking interval(0～12,700)(ms) |
Brightness |  |
Screen | Mode |  |
Custom mode | Column Row |
Background Color | Detail settings | Row R G B |
Slideshow | Start | Interval |
Stop |  |
Bar Code | Symbol | Data Type Error Correction Level Module Width Module Height DotX DotY QuietZone Hexadecimal: '\x00'～'\xff', Horizontal Tab(HT): '\t', Line Feed(LF): '\n', Carriage Return(CR): '\r', Back Slash: '\\' |
Clear Symbol |  |
Image | Register Download Image | Image File (in the same server) Keycode 1 Keycode 2 |
Display Download Image | Keycode 1 Keycode 2 DotX DotY Width Height |
Display NV Image | Keycode 1 Keycode 2 DotX DotY Width Height |
Clear Image |  |
Window(createTextArea) | Define display area | Window No. X-coordinate Y-coordinate Width Height Scroll Mode |
Discard display area setting | Window No. to discard |
Switch display area | Window No. to move |
Clear current display area |  |
Others | Display clock |  |
command |  |
Reset display |  |

Display Object Sample Code
Test display |