Device Setting
Connection settings | IP address Port Device ID Encryption Enable buffer |

Console

ePOS SDK Hybrid Printer Object
Common | Alignment |  |
Line Spacing |  |
Upside-down | Upside-down |
Text | Print Characters | Horizontal Tab(HT): '\t', Line Feed(LF): '\n', Carriage Return(CR): '\r', Back Slash: '\\' |
Language |  |
Font |  |
Smoothing | Enabled |
Double | Double-width Double-height |
Size | Width Height |
Style | White/Black Reverse Underline Emphasized Color |
X Position | Position |
Y Position | Position |
Paper Feed | By Unit | Units |
By Line | Lines |
Image | Raster Image | Image File (in the same server) Mode Brightness Color(Monochrome) Halftone(Monochrome) |
NV Logo | Keycode 1 Keycode 2 |
Bar Code | Bar Code | Data Type HRI Font Module Width Module Height Hexadecimal: '\x00'-'\xff', Horizontal Tab(HT): '\t', Line Feed(LF): '\n', Carriage Return(CR): '\r', Back Slash: '\\' |
Symbol | Data Type Error Correction Level Specify a constant definition Specify a numerical value Module Width Module Height Symbol Size Hexadecimal: '\x00'-'\xff', Horizontal Tab(HT): '\t', Line Feed(LF): '\n', Carriage Return(CR): '\r', Back Slash: '\\' |
Page Mode | Start |  |
Print Area | X Origin Y Origin Width Height |
Print Direction | Direction |
Print Position | X Position Y Position |
End |  |
Others | Paper Cutting | Type |
Drawer Kick-out | Connector ON Time |
40cplmode | Enable Disable |
Command | Hexadecimal: '\x00'-'\xff', Horizontal Tab(HT): '\t', Line Feed(LF): '\n', Carriage Return(CR): '\r', Back Slash: '\\' |

Hybrid Printer Object Sample Code -- target

Test print
lock/unlock |
MICR | ignoreerror | true false |
font |
timeout | (min)
Test print | Receipt print | Forced Transmission |
Slip print | timeout (min) |
Endorse print | timeout (min) |
Recovery | Forced Transmission |
Reset |
Status | Interval |
onstatuschange ononline, onoffline, onpoweroff oncoverok, oncoveropen onpaperok, onpaperend, onpapernearend ondrawerclosed, ondraweropen